{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":34,"n_cols":12,"rows_kept":34,"merged":[[0,0,0,6],[1,0,1,6],[33,0,33,4]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表"]
["项目名称：B北教学楼茶水间改造"]
["序号","拆除部分","计量单位","工程量","综合单价","合价","备注 "]
["一、","拆除部分"]
[null,"原吊顶","平方",{"v":19.8144,"d":"19.81"},null,0,"原轻钢龙骨+矿棉板"]
[null,"原房间设备","项",1,null,0,"原洗手台 大理石+钢架+台盆+支撑矮墙"]
[null,"已安装空调","项",1,null,0,"空调室内机保护"]
["二、","水电部分"]
[null,"线路","米",45,null,0,"开槽  BV4平方  由分支箱引入"]
[null,"暗盒","个",6,null,0,"安装+铺设"]
[null,"面板","个",6,null,0,"施耐德+安装"]
[null,"水管","米",4,null,0,"有原水头引入，开槽 暗辅"]
[null,"三角阀","个",1,null,0,"九牧+安装"]
[null,"不锈钢盆","套",1,null,0,"暗装+含笼头"]
[null,"下水管","米",2,null,0,"接原下水   地面会有修补",{"$nulls":4}," "]
["三、","墙面部分"]
[null,"墙面乳胶漆","平方",30.94,null,0,"修补，批一遍，打磨，立邦乳胶漆"]
[null,"墙面木工板打底","平方",16.78,null,0," 墙面挂大理石，木工板打底"]
[null,"800*800砖干挂","平方",16.78,null,0,"加工，云石胶.人工.损耗"]
[null,"45度倒角","米",6,null,0,"加工"]
["四、","吊顶部分"]
[null,"集成吊顶","平方",19.81,null,0,"600*600 铝板吊顶加厚"]
[null,"600*600平板灯","套",4,null,0,"600*600平板灯雷士  含安装"]
[null,"线路布置","平方",19.81,null,0]
["五、","设备部分"]
[null,"地柜","米",4.16,null,0,"两个抽屉+平板门+多层板+定制门"]
[null,"通体柜","米",1,null,0]
[null,"台面","米",4.16,null,0,"石英石"]
[null,"吊柜","米",4.16,null,0,"平板门+定制"]
[null,"运费"]
[null,"楼层费"]
[]
[]
["合计",{"$nulls":4},0]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}